Integrated Intel Celeron 1037 dual core processor(1.8GHz)

Intel NM70 express chipset

Integrated Intel HD graphics, supports VGA, HDMI and LVDS video output

SO-DIMM DDR3 memory slot, supports 1333/1066 memory

Onboard 2 mini-PCIE slots, supports SSD/Wifi/3G modules

Supports Max. 10 RS232 Serial ports, COM2/3 supports RS422/485 modes

Onboard 2 RTL8111E 1000M Ethernet controllers, supports Wake On LAN

Integrated Realtek ALC662 6 channel high definition audio controller
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1. Motherboard Front View
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2. I/O Panel Front View
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3. I/O Panel Side View
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4. Memory Side View
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II. ITX-M847_A18 VER:1.2 Motherboard Photo

1. Motherboard Front View
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2. I/O Panel Front View
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3. I/O Panel Side View
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4. Memory Slot Side View
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	Product Model
	ITX-M847_A10(A18) VER: 1.2

	CPU
	Onboard Intel 1037U dual core 22nm processor (1.8Ghz)

	Chipset
	Intel NM70 Chipset

	Memory
	Dual channel SO-DIMM DDR3 memory slots, supports 1333/1066 Mhz, Max. 16GB.

ITX-M847_A18 supports 1 memory slot, Max. 8GB

	Video
	Integrated Intel HD graphics core
Provides VGA, HDMI and dual channel 24 bit LVDS video output

Supports HDMI/VGA synchronization/asynchronization

Supports LVDS/VGA synchronization/asynchronization

Supports LVDS/HDMI synchronization/asynchronization

	Expansion Slot
	1 x mini PCI-e slot, supports wifi/3G module
1 x MSATA slot, suppports SSD/Wifi, SSD Max. transfer rate 6Gbps

	LAN
	2 x RTL8111E 1000M Ethernet controller, supports Wake On Lan, PXE booting.
1 x RTL8105E 100M Ethernet controller(ITX-M847_A18 adapts)

	Storage
	3 x SATAII HDD interface, Max. transfer rate 3Gbps

	Audio
	Onboard Realtek ALC662 6 channel high fidelity audio chip, supports MIC, line out.

	Rear I/O panel
	1 x PS/2 keyboard and mouse connector
1 x DB9 COM port, PIN9 with electrification function

1 x LPT port

1 x DB15 VGA port

2 x RJ-45 LAN ports

4 x USB 2.0 ports

1 x audio I/O interface(MIC and line out) 

	Internal I/O interface
	9 x COM, COM2 and COM3 support RS485/422 (ITX-M847_A18 supports 5 internal COM)
1 x LVDS connector, supports dual channel 24 bit LCD, 2 x15-pin
1 x HDMI connector, 2 x 8-pin

1 x VGA1 connector, 2 x 5-pin

4 x USB 2.0 connectors

1 x audio connector

1 x FP1 front panel function button and indicator light header, 2 x 5-pin

1 x TX-RXCOM RS422/485 header, 2 x 4-pin

1 x PS/2 mouse and keyboard connector, 6-pin

1 x SIM slot

	Fan connector
	1 x CPU Fan connector and 1 x System Fan connector, 4-pin

	GPIO
	Supports 4 channel GPIO

	BIOS
	AMI 32MB Flash ROM

	Watch Dog
	Supports hardware reset function(256 level, 0-255 seconds)

	PSU
	ATX power supply

	Working Temp
	-10℃～60℃

	Storing Temp
	-20℃～70℃

	Working Humidity
	5%-95% relative humidity, non-condensing

	Dimension
	170mm x 170mm

Mini ITX form factor


